

SURFACING SOLUTION		Guide Specifications in CSI Format
www.SurfacingSolution.com		Tel. 800-964-6726

SECTION 062200
FLEXIBLE WOOD TAMBOUR PANELS
GENERAL
SUMMARY
Provide flexible wood tambour panels of the following types:
Solid wood tambours.
Veneer tambours.
Related Sections:  Coordinate with the following as applicable: 
Section 064000 - Architectural Woodwork for other woodwork.
Section 092116 - Gypsum Board Assemblies for substrate.
SUBMITTALS
Product Data:  Submit manufacturer's literature including product characteristics and accessories.
Shop Drawings:  Submit diagram showing layout of pattern and configuration, including details of perimeter conditions and mounting.
Verification Samples:  Submit samples of materials selected for use to verify profile, color, and finish.
QUALITY ASSURANCE
Manufacturer:  Minimum of 5 years experience manufacturing similar products.
Installer:  Minimum of 2 years experience installing similar products.
Field Measurements:  To the greatest extent practical, take field measurements prior to fabrication.
DELIVERY, STORAGE AND HANDLING
Deliver materials and products in unopened factory labeled packages. Store and handle in strict compliance with manufacturer's instructions and recommendations.
PRODUCTS
MANUFACTURER
Basis-of-Design Manufacturer:   Surfacing Solution, 2480 Chaska Blvd., Chaska, MN 55318.  Tel 800.964-6727.  Fax 800.964.0630.  www.SurfacingSolution.com.
SOLID WOOD TAMBOUR PANELS
Basis of Design:  Solid Wood Tambour by Surfacing Solution.
Nominal Sheet Width:  [12 inches (305 mm)] [16 inches (406 mm)].
Nominal Sheet Length:  [36 inches (914 mm)] [48 inches (1219 mm)] [60 inches (1524 mm)] [72 inches (1829 mm)] [84 inches (2134 mm)] [96 inches (2438 mm)] [108 inches (2743 mm)] [120 inches (3048 mm)] [132 inches (3353 mm)] [144 inches (3658 mm)].
Species:  [Red Oak] [Cherry] [Walnut] [Ash] [Maple] [Alder] [Red Grandis] [Poplar (paint grade] [White Oak] [_____].
Profiles:
T374:  Slat width of 3/4 inches (19 mm) and height of 7/32 inches (5.6 mm).
T375:  Slat width of 3/4 inches (19 mm) and height of 11/32 inches (8.7 mm).
T378:  Slat width of 3/4 inches (19 mm) and height of 3/8 inches (9.5 mm).
T383:  Slat width of 3/4 inches (19 mm) and height of 5/16 inches (7.9 mm).
T311:  Slat width of 3/4 inches (19 mm) and height of 3/8 inches (9.5 mm).
T412:  Slat width of 1 inch (25 mm) and height of 5/16 inches (7.9 mm).
T474:  Slat width of 1 inch (25 mm) and height of 1/4 inches (6.4 mm).
T478:  Slat width of 1 inch (25 mm) and height of 1/2 inches (13 mm).
T493:  Slat width of 1 inch (25 mm) and height of 1/2 inches (13 mm).
T475:  Slat width of 1 inch (25 mm) and height of 1/2 inches (13 mm).
T593:  Slat width of 1-1/4 inches (32 mm) and height of 5/8 inches (16 mm).
T505:  Slat width of 1-1/4 inches (32 mm) and height of 3/8 inches (9.5 mm).
T530:  Slat width of 1-1/4 inches (32 mm) and height of 3/16 inches (4.8 mm).
T611:  Slat width of 1-1/2 inches (38 mm) and height of 3/8 inches (9.5 mm).
T674:  Slat width of 1-1/2 inches (38 mm) and height of 3/16 inches (4.8 mm).
T675:  Slat width of 1-1/2 inches (38 mm) and height of 11/32 inches (8.7 mm).
T655:  Slat width of 1-1/2 inches (38 mm) and height of 1/2 inches (13 mm).
T678:  Slat width of 1-1/2 inches (38 mm) and height of 3/4 inches (19 mm).
T676:  Slat width of 1-1/2 inches (38 mm) and height of 3/4 inches (19 mm).
T624:  Slat width of 1-1/2 inches (38 mm) and height of 3/4 inches (19 mm).
T324A:  Slat width of 3/4 inches (19 mm) and height of 3/4 inches (19 mm).
T484A:  Slat width of 1 inch (25 mm) and height of 5/8 inches (16 mm).
T684A:  Slat width of 1-1/2 inches (38 mm) and height of 1 inch (25 mm).
T693:  Slat width of 1-1/2 inches (38 mm) and height of 3/4 inches (19 mm).
T878:  Slat width of 2 inches (51 mm) and height of 1 inch (25 mm).
T864:  Slat width of 2 inches (51 mm) and height of 1/4 inch (6.4 mm).
T324B:  Slat width of 3/4 inches (19 mm) and height of 3/4 inches (19 mm).
T484B:  Slat width of 1 inch (25 mm) and height of 5/8 inches (16 mm).
T684B:  Slat width of 1-1/2 inches (38 mm) and height of 1 inch (25 mm).
T1164:  Slat width of 3-1/2 inches (89 mm) and height of 1/4 inch (6.4 mm).
Field Finish:  [Stain and clear coat polyurethane] [Clear] [Natural oil] [Paint].
WOOD VENEER TAMBOUR PANELS
Basis of Design:  Real Wood Veneer Tambour by Surfacing Solution.
Panel Size:  4 x 8 feet (1219 x 2438 mm).
Core Material:  MDF or black PVC.
Profile 231:
Slat Width:  1/2 inch (13 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Smooth.
Species:  [Red Oak] [Maple] [Brushed Aluminum] [_____].
Profile 331:
Slat Width:  3/4 inch (19 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Smooth.
Species:  [Red Oak] [Maple] [White Oak] [Cherry] [Grey Stained White Oak] [Purple Heart] [Teak] [Brushed Aluminum] [_____].
Profile 332:
Slat Width:  3/4 inch (19 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Wire brushed.
Species:  [White Ash] [Teak] [African Wenge] [Red Oak] [White Oak] [Elm] [_____].
Profile 431:
Slat Width:  1 inch (25 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Smooth.
Species:  [Apple] [Maple] [Rose Wood] [Weathered Grey Oak] [_____].
Profile 432:
Slat Width:  1 inch (25 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Wire brushed.
Species:  [Sycamore] [_____].
Profile 631:
Slat Width:  1-1/2 inches (38 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Smooth.
Species:  [White Oak] [Red Oak] [Maple] [_____].
Profile 831:
Slat Width:  2 inches (51 mm).
Slat Height:  5/32 inch (4.0 mm).
Texture:  Smooth.
Species:  [Red Oak] [_____].
Field Finish:  [Stain and clear coat polyurethane] [Clear] [Natural oil] [Paint].
EXECUTION
EXAMINATION
Examine substrates for compliance with requirements for installation tolerances and other conditions affecting performance.  Proceed with installation only after unsatisfactory conditions have been corrected.
INSTALLATION
Install products in strict accordance with manufacturer’s instructions, approved submittals and in proper relationship to adjacent construction.
Clean substrate of dirt and bond breaking substances prior to beginning installation.
Acclimatize panels at the installation site for a minimum of 48 hours prior to installation.
Roll tambour panels in accordance with manufacturer’s instructions to properly space slats.
Follow manufacturer’s recommendations for adhesives and mounting devices.
Replace damaged or defaced products prior to Substantial Completion.
CLEANING
Clean surfaces to remove soiling, stains, dust, and dirt using materials acceptable to manufacturer.
Leave installation area clean and free of residue and debris resulting from work of this Section.
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