[image: C:\Users\Jeramey\Pictures\CUT SHEETS FINALIZED\surfacingsolution logo.jpg]

APPROVED ASSEMBLY OF SOLID HARDWOOD FLOOR WITH PLYWOOD
• Make sure subfloor is clean, dry, and flat. If some areas require fill
patching or leveling use a self leveling underlayment.
• Must check subfloor for excessive moisture. If a moisture barrier is
needed use a suitable vapor barrier or moisture sealer.
• Loose lay Acoustical Decoupler on subfloor, do not glue.
• Make sure Acoustical Decoupler covers the perimeter of the
entire subfloor and around any protrusions.
• Always install black side down.
• The Acoustical Decoupler seams must be placed tightly
together and taped with duct tape.
• Loose lay the first layer of plywood (3/4”) on Acoustical
Membrane.
• Install second layer of plywood (1/2”) on top of the first layer of
plywood. The top layer of plywood must be perpendicular to the
bottom layer, joints gapped and offset, top sheet glued (full coverage,
non water based adhesive) to bottom sheet. The top layer fastened with
1” #8 flat head wood screws every 12” with no penetration into the
Acoustical Membrane.
• Nail down hardwood floor on the plywood without penetrating the
Acoustical Membrane.
THIS INSTALLATION WILL CREATE A FLOATING HARDWOOD
FLOOR ON PLYWOOD ASSEMBLY OVER ACOUSTICAL
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